* RLS_NO *
r10.0
* PRE_PROCESSING * MAKE_SYSTEM_MATRICES * PRE_CONDITIONING *
     1       1
* SOLVE_EQUATION * POST_PROCESSING *
       1                  1
* STATIC * STEP * AC * TRANSIENT * DISPLACEMENT * NON_LINEAR *
    1       0     0       0          0           0
* POTENTIAL *
    0
* TREE_GAUGE *
   -1                    1
* NODE_ORDER * EDGE_ORDER *  METRIC_MOD * QUAD_TRI * CALC_IND * THIN_ELEM * NO_PARALLEL *
         1                      1                     0                       0                0     0     2
* ICCG_CONV * ACCEL_FACTOR * DIV_FACTOR * DIV_ITERATIONS * SOLVER *
    1.e-8        1.            10.          10             0
* NON_LINERAR_CONV * RELAXATION * NO_ITERATIONS *
    1.e-3             1.0            20
* POINTS_IN_1D * POINT_IN_TRIANGLE * MAT_POINTS * 
         3               7               0
* INITIAL_STEP *
     -1
* NO_STEPS * INITIAL_TIME(s) *  DELTA_TIME(s) *
      1          0.0             1.0 
* INITIAL_STEP * LAST_STEP * STEP_INTERVAL * TIME_DIFFERENCE *
       1              1          1                3
* INPUT_MESH_FILE *  UNIT  * NO_MESH *  MESHLESS *
        5                        0           0                 1
* POST_DATA_FILE * ELEM_OUT * NODE_OUT *NUMBER_OUTPUT_MATS * AVERAGE * WIDE * SUF_OPTION *
        5                            0                   0                    0                            0               1
* MESH * CURRENT * MAGNETIC * FORCE_J_B* FORCE_NODAL * DISPLACEMENT * ELEMENT *
   1            0         0           0          0             0            0
*   MESH   *   A   *   V   *   B   *   B_INTEG *    J_Q  *
     0             0             0       0        1           0
*  Q_AVERAGE *  Q_TOTAL  *  MAG_FLUX  * CUR_FLUX *
        0         0            0            0
* FORCE_J_B * FORCE_NODAL *
        0         0
* XSYMMETRY * YSYMMETRY * ZSYMMETRY * ROTATION *
      1                     1                     -1                 1
* NO_POINTS * NO_MAT_IDS * NO_COIL_SERIES * INTEG_OPT *  MESH_INPUT *
         0                   0                  1                        1                      1
*   XP(m) *    YP(m)  *      ZP(m)  *
* MAT_IDS *
*     15
* COIL_SERIES *
       1
* GEOMETRY * DELTA_Z(m) or DETLA_THETA(deg)*
     0         1.0
*COORDINATE * NO_COORDINATES *
COORDINATE         0
* FAR_BOUNDARY_CONDITION 
        0                     0               
* DISTANCE_JUDGE(m) * Distance for judgement (m)
      1.e-3
* NO_BN0_PLANES *
    2
*     CX        *       CY        *      CZ       *      C(m)   *
      1.0               0.0              0.0             0.0
      0.0               1.0              0.0             0.0
* NO_HT0_PLANES *
    1
*     CX        *       CY        *      CZ       *      C(m)   *
      0.0               0.0              1.0             0.0
* NO_A0_LINE *
    0
* CYCLIC     *  SYMMETRICITY *  SLIDE_NDIV *  SLIDE_MAT *
     0               1             0          11
* NO_MAT_IDS *  EXTEND_TOTAL *  NO_SMAT_IDS 
     0               0            0
*SOURCE *
SOURCE  
*COIL   * SERIES_NO  *  TIME_ID  *  NO_ELEMENTS * MOTIN_ID *
* COILの定義、対象条件を考慮せず全体で入力します。８要素からなります。
COIL         1            0          11             0  
*LINE_APPROX * LIMIT *
LINE_APPROX   10000.
*GCE    * CURRENT(A)*
* GCEは直線部
GCE        100.
*            XS(m)  *   YS(m)  *  ZS(m)  *  XE(m)  *  YE(m)  *  ZE(m)  *
           0.0875      -0.05      0.0       0.0875    0.05       0.0
*            W1X(m) *   W1Y(m) *  W1Z(m) *  W2X(m) *  W2Y(m) *  W2Z(m) *
           0.0          0.0       0.05      0.0125    0.0        0.0
*GCE    * CURRENT(A)*
GCE        100.
*            XS(m)  *   YS(m)  *  ZS(m)  *  XE(m)  *  YE(m)  *  ZE(m)  *
           0.05         0.0875    0.0      -0.05      0.0875    0.0
*            W1X(m) *   W1Y(m) *  W1Z(m) *  W2X(m) *  W2Y(m) *  W2Z(m) *
           0.0          0.0       0.05      0.0       0.0125    0.0
*GCE    * CURRENT(A)*
GCE        100.
*            XS(m)  *   YS(m)  *  ZS(m)  *  XE(m)  *  YE(m)  *  ZE(m)  *
          -0.0875       0.05      0.0      -0.0875   -0.05       0.0
*            W1X(m) *   W1Y(m) *  W1Z(m) *  W2X(m) *  W2Y(m) *  W2Z(m) *
           0.0          0.0       0.05     -0.0125    0.0        0.0
*GCE    * CURRENT(A)*
GCE        100.
*            XS(m)  *   YS(m)  *  ZS(m)  *  XE(m)  *  YE(m)  *  ZE(m)  *
          -0.05        -0.0875    0.0       0.05     -0.0875    0.0
*            W1X(m) *   W1Y(m) *  W1Z(m) *  W2X(m) *  W2Y(m) *  W2Z(m) *
           0.0          0.0       0.05      0.0      -0.0125    0.0
*ARC    *  CURRENT(A)  *
ARC       100.
*          X(m)  *  Y(m)  *   Z(m)  * RADIUS(m)* AXIAL_W(m)*RADIAL_W(m)*
          0.05     0.05      0.0      0.0375         0.1        0.025
*          ALPHA(deg)* BETA(deg) * PHI1(deg)   * PHI2(deg) *
          0.0      0.0       0.0      90.
*ARC    *  CURRENT(A)  *
ARC       100.
*          X(m)  *  Y(m)  *   Z(m)  * RADIUS(m)* AXIAL_W(m)*RADIAL_W(m)*
         -0.05     0.05      0.0      0.0375         0.1        0.025
*          ALPHA(deg)* BETA(deg) * PHI1(deg)   * PHI2(deg) *
          0.0      0.0       90.     180.
*ARC    *  CURRENT(A)  *
ARC       100.
*          X(m)  *  Y(m)  *   Z(m)  * RADIUS(m)* AXIAL_W(m)*RADIAL_W(m)*
         -0.05    -0.05      0.0      0.0375         0.1        0.025
*          ALPHA(deg)* BETA(deg) * PHI1(deg)   * PHI2(deg) *
          0.0      0.0      180.      270.
*ARC    *  CURRENT(A)  *
ARC       100.
*          X(m)  *  Y(m)  *   Z(m)  * RADIUS(m)* AXIAL_W(m)*RADIAL_W(m)*
          0.05    -0.05      0.0      0.0375         0.1        0.025
*          ALPHA(deg)* BETA(deg) * PHI1(deg)   * PHI2(deg) *
          0.0      0.0      270.      360.
*GCE    * CURRENT(A)*
GCE-        50.
*            XS(m)  *   YS(m)  *  ZS(m)  *  XE(m)  *  YE(m)  *  ZE(m)  *
           0.0875          0.0      0.025       0.0875    0.05       0.025
*            W1X(m) *   W1Y(m) *  W1Z(m) *  W2X(m) *  W2Y(m) *  W2Z(m) *
           0.0          0.0       0.025      0.0125    0.0        0.0
*  NDIV * INT_X * INT_Y * INT_Z *
        1       5          5         3
*ARC    *  CURRENTA)  *
ARC-       50.
*          X(m)  *  Y(m)  *   Z(m)  * RADIUS(m)* AXIAL_W(m)*RADIAL_W(m)*
          0.05     0.05      0.025      0.0375         0.05        0.025
*          ALPHA(deg)* BETA(deg) * PHI1(deg)   * PHI2(deg) *
          0.0      0.0       0.0      90.
*  NDIV * INT_X * INT_Y * INT_Z *
         1         5         5         3
*GCE    * CURRENT(A)*
GCE-        50.
*            XS(m)  *   YS(m)  *  ZS(m)  *  XE(m)  *  YE(m)  *  ZE(m)  *
           0.05         0.0875    0.025         0.00      0.0875    0.025
*            W1X(m) *   W1Y(m) *  W1Z(m) *  W2X(m) *  W2Y(m) *  W2Z(m) *
           0.0          0.0       0.025      0.0       0.0125    0.0
*  NDIV * INT_X * INT_Y * INT_Z *
       1          5         5         3
*END of COIL *
END
*CIRCUIT *
CIRCUIT
* NO_SERIES * NO_POWER_SUPPLIES *  REGION_FACTOR *
        1                1                   8.
* SERIES_IDS *
        1
* SERIES_EXTERNAL_INDUCTANCE *
        0.0
* SERIES_EXTERNAL_RESISTANCE *
        0.0
*  CONNECTION_MATRIX *
        1.0 
* PS_ID    *    TYPE  * TIME_ID *   INITIAL_CURRENT *
     1            0         1                0.0   
* END 0f CIRCUIT
END
*END of SOURCE *
END
* NO_DATA *
      1
* TIME_ID * OPTION *
      1     0
*   C0    *   C1    *   C2    *   C3     *   C4     *  C5    *   C6    *
    10.        0.0       0.0       0.0        0.0       0.0       0.0
*  TEXP   *   TCYCLE  *
    0.0       0.00