*RLS_NO
r10.0
* PRE_PROCESSING * MAKE_SYSTEM_MATRICES  *
        1                    1
* SOLVE_EQUATION * POST_PROCESSING *
         1          1
* STATIC * STEP * AC * TRANSIENT * DISPLACEMENT * NON_LINEAR * TEMP_DEPEND * STEADY_CURRENT*
      0       0          0          1                  1            0            0            0
* POTENTIAL * NODAL_FORCE_METHOD * PHI_OPTION * FIXED_COORDINATE *
    2                0                   0                0
* TREE_GAUGE * REGULARIZATION * SCALING * RENUMBERING * LINE_SEARCH *
   -1               1               0          0               0
* NODE_ORDER * EDGE_ORDER *  METRIC_MOD * QUAD_TRI * CALC_IND *  THIN_ELEM  *
              1              1                      0                    0                0                  0
* ICCG_CONV * ACCEL_FACTOR * DIV_FACTOR * DIV_ITER * SOLVER * THETA * THETA_NETWORK * THETA_MOTION *
*    1e-006             1.           100.          100         0    0.6666667        0.5        0.5
    1e-006             1.            100.          100         0     1.0        0.5        0.5
* NON_LINERAR_CONV * RELAXATION * NO_ITERATIONS * INIT_OPTION * ICCG_CONV_RATIO *  CHECK_B *
     0.001                  1           20          0          0.001                   1
* POINTS_IN_1D * POINT_IN_TRIANGLE * MAT_POINTS *
         3               7               1
* INITIAL_STEP * DATA_TYPE  * INITIAL_PHASE * MULTI *
    -1           0               0        0
* NO_STEPS * INITIAL_TIME(s) *  DELTA_TIME(s) * NO_DATA * CYCLIC *N_CORRECT *
     101             0.        8.3333333333e-5             0        15         15
* INITIAL_STEP * LAST_STEP *  STEP_INTERVAL * TIME_DIFFERENCE * RESTART_FILE_OPTION *
     1                    241             1             3                  0
* INPUT_MESH_FILE *  UNIT  *
        5            0
* POST_DATA_FILE * ELEM_OUT * NODE_OUT *NUMBER_OUTPUT_MATS * AVERAGE * WIDE * SUF_OPTION *
       0             1         0           0                0            0          0 *     11
* MESH * CURRENT * MAGNETIC * FORCE_J_B* FORCE_NODAL * DISPLACEMENT * ELEMENT *  HEAT * MAGNETIZATION *
      1           1                1                    0                  0                     1           0         0        0
*   MESH   *   A   *   V   *   B   *   B_INTEG *    J_Q  *
       0       0     0       0        0         0
*  Q_AVERAGE *  HEAT  *  MAG_FLUX  * CUR_FLUX *
       0          1        0          0
* FORCE_J_B * FORCE_NODAL *  MAGNETIC_ENERGY 
    0           0         0
* GEOMETRY * DELTA_Z(m) or DELTA_THETA(deg)*
     0                      1
* COORDINATE * NO_COORDINATES *
COORDINATE  8
* COORD_ID * TYPE   *    X0    *    Y0    *    Z0   *
       1            1             0.2      0.00          0
*                   *   EX_X   *   EX_Y   *   EX_Z  *
                          1          0          0
*                   *   EZ_X   *   EZ_Y   *   EZ_Z  *
                          0          0          1 
* COORD_ID * TYPE   *    X0    *    Y0    *    Z0   *
       2            1             0.14142136       0.14142136           0
*                   *   EX_X   *   EX_Y   *   EX_Z  *
                          0.7071678       0.7071678          0
*                   *   EZ_X   *   EZ_Y   *   EZ_Z  *
                          0          0          1 
* COORD_ID * TYPE   *    X0    *    Y0    *    Z0   *
       3            1             0.      0.2          0
*                   *   EX_X   *   EX_Y   *   EX_Z  *
                          0          1.          0
*                   *   EZ_X   *   EZ_Y   *   EZ_Z  *
                          0          0          1 
* COORD_ID * TYPE   *    X0    *    Y0    *    Z0   *
       4            1            -0.14142136       0.14142136           0
*                   *   EX_X   *   EX_Y   *   EX_Z  *
                         -0.7071678       0.7071678          0
*                   *   EZ_X   *   EZ_Y   *   EZ_Z  *
                          0          0          1 
* COORD_ID * TYPE   *    X0    *    Y0    *    Z0   *
       5            1            -0.2      0.00          0
*                   *   EX_X   *   EX_Y   *   EX_Z  *
                         -1          0          0
*                   *   EZ_X   *   EZ_Y   *   EZ_Z  *
                          0          0          1 
* COORD_ID * TYPE   *    X0    *    Y0    *    Z0   *
       6            1            -0.14142136      -0.14142136           0
*                   *   EX_X   *   EX_Y   *   EX_Z  *
                         -0.7071678      -0.7071678          0
*                   *   EZ_X   *   EZ_Y   *   EZ_Z  *
                          0          0          1
* COORD_ID * TYPE   *    X0    *    Y0    *    Z0   *
       7            1            0.0      -0.20          0
*                   *   EX_X   *   EX_Y   *   EX_Z  *
                        0               -1.          0
*                   *   EZ_X   *   EZ_Y   *   EZ_Z  *
                          0          0          1 
* COORD_ID * TYPE   *    X0    *    Y0    *    Z0   *
       8            1            0.14142136      -0.14142136           0
*                   *   EX_X   *   EX_Y   *   EX_Z  *
                         0.7071678      -0.7071678          0
*                   *   EZ_X   *   EZ_Y   *   EZ_Z  *
                          0          0          1
* FAR_BOUNDARY_CONDITION * IMP_BOUNDARY *
     0
* DISTANCE_JUDGE(m) * Distance for judgement (m)
           0.00001
* NO_BN0_PLANES *
    0
* NO_HT0_PLANES *
    0
* NO_AT_LINES *
    0
*  CYCLIC  *  SYMMETRICITY *
    2         0
    45.
* NO_MAT_IDS *  EXTEND_TOTAL *  NO_SMAT_IDS
       2                1                 0
* MAT_ID  *  POTENTIAL * B_H_CURVE_ID   *  SIGMA  *       MU       * PACKING *
     11        0           0                 5.e7             1         1
     12        1           0                    0             1         1
*  50.       1
*      12
*SOURCES Definitions*
SOURCE
*COIL * SERIES_NO * TIME_ID * NO_ELEMENTS * MOTION_ID * IN_ROTOR *
COIL             1              1              8                     1          0
COORDID	   1
LOOP           1.            0.05     -0.04    0.02   0.02    
COORDID	   2
LOOP          1.            0.05     -0.04    0.02   0.02    
COORDID	   3
LOOP           1.            0.05     -0.04    0.02   0.02    
COORDID	   4
LOOP          1.            0.05     -0.04    0.02   0.02    
COORDID	  5
LOOP           1.            0.05     -0.04    0.02   0.02    
COORDID	   6
LOOP          1.            0.05     -0.04    0.02   0.02    
COORDID	   7
LOOP           1.            0.05     -0.04    0.02   0.02    
COORDID	   8
LOOP          1.            0.05     -0.04    0.02   0.02    
END
* END of Source
END
* NO_DATA *
	  2
* TIME_ID * OPTION *
      1     0
*   C0    *   C1    *   C2    *   C3     *   C4     *  C5    *   C6    * 
    1.e5        0.0       0.0       0.0        0.0       0.0       0.0
*  TEXP   *   TCYCLE  *
    0.0       0.00
* TIME_ID * OPTION *
     2     0
*   C0    *   C1    *   C2    *   C3     *   C4     *  C5    *   C6    * 
      0.        360.e2       0.0       0.0        0.0       0.0       0.0
*  TEXP   *   TCYCLE  *
    0.0       0.0
MOTION     1
   1   0  0  0  2 0
    0   