*RLS_NO
r10.2
* PRE_PROCESSING * MAKE_SYSTEM_MATRICES * PRE_CONDITIONING *
       1                      1       
* SOLVE_EQUATION * POST_PROCESSING *
        1                     1
* STATIC * STEP * AC * TRANSIENT * DISPLACEMENT * NON_LINEAR * STEADY_CURRENT*
     0               0      0                1                  0                    1          0
* POTENTIAL *
    2
* TREE_GAUGE * REGULARIZATION * RENUMBERING * SCALING * LINE_SERACH * MATRIX_ASYMMETRICITY *
   -1                           0                               0                 0                1
* ORDER_OF_SHAPE_FUNCTIONS *
              1
* ICCG_CONV * ACCEL_FACTOR * DIV_FACTOR * DIV_ITER * SOLVER * THETA * THETA_NETWORK * THETA_MOTION *
    1e-008          0                            10                    10         0              1.0       1.0        0.5
* NON_LINERAR_CONV * RELAXATION * NO_ITERATIONS * INIT_OPTION * ICCG_CONV_RATIO * CHECK_B * DELTA_A *
     1.0e-003                    1.0                   20                  0                          1.e-3                     -1.e-2
* POINTS_IN_1D * POINT_IN_TRIANGLE * MAT_POINTS *
         3               7               1
* INITIAL_STEP * DATA_TYPE  * INITIAL_PHASE *
      -1           0             0.000000000
* NO_STEPS * INITIAL_TIME(s) *  DELTA_TIME(s)*
   101                   0                  0.0005                0             0         20
* INITIAL_STEP * LAST_STEP *  STEP_INTERVAL * TIME_DIFFERENCE * RESTART_FILE_OPTION *
            1           100         1             3                  0
* INPUT_MESH_FILE *  UNIT  *
         5            1
* POST_DATA_FILE * ELEM_OUT * NODE_OUT *NUMBER_OUTPUT_MATS * AVERAGE * WIDE * SUF_OPTION *
       5                           1               0                    1                0            0          0
       4
* MESH * CURRENT * MAGNETIC * FORCE_J_B* FORCE_NODAL * DISPLACEMENT * ELEMENT *  HEAT *
   1                1              1          0             0             0            0      1
*   MESH   *   A   *   V   *   B   *   B_INTEG *    J_Q  *
       0       0     0       0        0         0
*  Q_AVERAGE *  HEAT  *  MAG_FLUX  * CUR_FLUX *
       0                      1        0          0
* FORCE_J_B * FORCE_NODAL *  MAGNETIC_ENERGY 
    0           0         0
* GEOMETRY * DELTA_Z(m) or DELTA_THETA(deg)*
     0                      1
* COORDINATE * NO_COORDINATES *
COORDINATE  0
* FAR_BOUNDARY_CONDITION * IMP_BOUNDARY *
     0
* DISTANCE_JUDGE(m) * Distance for judgement (m)
    9.9999997e-005
* NO_BN0_PLANES *
    2
*     CX        *       CY        *      CZ       *      C(m)   *
 1.0000000e+000      0.0000000e+000     0.0000000e+000    0.0000000e+000
 0.0000000e+000      1.0000000e+000     0.0000000e+000    0.0000000e+000
* NO_HT0_PLANES *
    1
*     CX        *       CY        *      CZ       *      C(m)   *
 0.0000000e+000      0.0000000e+000     1.0000000e+000    0.0000000e+000
* NO_AT_LINES *
    0
*  CYCLIC  *  SYMMETRY  *  SLIDE_NDIV  *  SLIDE_MAT  *
    0         1            0.0000000e+000         11
* NO_MAT_IDS *  EXTEND_TOTAL *  NO_SMAT_IDS
         4               0                 0
* MAT_ID  *  POTENTIAL * B_H_CURVE_ID *  SIGMA  *  MU   * PACKING *
       2             0               1              7.505e+006        1.        1.0000000
       4             0               1              7.505e+006        1.        1.0000000
* MAT_ID  *  POTENTIAL * B_H_CURVE_ID *  SIGMA  *  MU   * PACKING *
       1            0               0                    0               1        1.0000000
* MAT_ID  *  POTENTIAL * B_H_CURVE_ID *  SIGMA  *  MU   * PACKING *
       7             0               0                    0               1        1.0000000
*SOURCES Definitions*
SOURCE
*SDEFCOIL  *SERIES_NO *NO_PARTS * IN_ROTOR *
SDEFCOIL           1                 1                 0
* MAT_ID * S_MAT_ID1 * S_MAT_ID2 * S_MAT_ID3 * S_MAT_ID4 * CURRENT *  SIGMA  *
     7 	 11   12   13  14                1500.           5.e7
* NETWORK *
NETWORK    8.0     0
FEM    1     1     2    1
VPS    2     2     1     1    0.e-3
END
END
* NO_DATA *
	  1
* TIME_ID *	OPTION	*
	    1         0
*   1000.          0.01   -90.
*   C0    *   C1    *   C2    *   C3     *   C4     *  C5    *   C6    * 
     1000.         0.      0.0       0.0        -1000.0   0.0        0.0      
*  TEXP   *   TCYCLE  *
   0.0           0.01
* TIME_ID *	OPTION	*
*	    1         2	 
*1.       0.001       0.
** 20. B_H curves ******************************************************
* NO_CURVES *
     1
* BH_CURVE_ID * NO_DATA *
     1             39       
*   H_AT/M     *      B_T    *
0.0     0.0
27.     0.01
58.     0.025
100.    0.05
153.    0.10
185.    0.15
205.    0.20
233.    0.30
255.    0.40
285.    0.50
320.    0.60
355.    0.70
405.    0.80
470.    0.90
555.    1.00
673.    1.10
836.    1.20
1065.   1.30
1220.   1.35
1420.   1.40
1720.   1.45
2130.   1.50
2670.   1.55
3480.   1.60
4500.   1.65
5950.   1.70
7650.   1.75
10100.  1.80
13000.  1.85
15900.  1.90
21100.  1.95
26300.  2.00
32900.  2.05
42700.  2.10
61700.  2.15
84300.  2.20
110000. 2.25
135000. 2.30
6262000.  10.0
