* RLS_NO *
r10.1
**** Execution module: EMSOL  r10.2.2  October 7, 2008 ****
* PRE_PROCESSING * MAKE_SYSTEM_MATRICES *
       1                  1                   
* SOLVE_EQUATION * POST_PROCESSING *
       1                  1
* STATIC * STEP * AC * TRANSIENT * DISPLACEMENT * NON_LINEAR * TEMP_DEPEND * STEADY_CURRENT *
    0       0     0       1          0           0
* POTENTIAL * NODAL_FORCE_OPTION * PHI_OPTION * FIXED_COODINATE *
    0
* TREE_GAUGE * REGULARIZATION * RENUMBERING * SCALING * LINE_SERACH * MATRIX_ASYMMETRICITY *
   -1 
* NODE_ORDER * EDGE_ORDER *  METRIC_MOD * QUAD_TRI * CALC_IND *  THIN_ELEM *
         1
* ICCG_CONV * ACCEL_FACTOR * DIV_FACTOR * DIV_ITERATIONS * SOLVER * THETA * THETA_NETWOEK * THETA_MOTION *
    1.e-6                 0.                      10.                    10                        0           0.5          0.5
* NON_LINERAR_CONV * RELAXATION * NO_ITERATIONS * INIT_OPTION * ICCG_CONV_RATIO * CHECK_B * DELTA_A *
    1.e-3             1.0            20
* POINTS_IN_1D * POINT_IN_TRIANGLE * MAT_POINTS * 
         3               7               0
* INITIAL_STEP * DATA_TYPE * INITIAL_PHASE *
    -1
* NO_STEPS * INITIAL_TIME(s) *  DELTA_TIME(s) * NO_DATA * CYCLE *N_CORRECT *
  201         0.              0.05e-3        0       0       40
* INITIAL_STEP * LAST_STEP * STEP_INTERVAL * TIME_DIFF * RESTART_FILE_OPTION * CONT *
       1          1000          1                3
* INPUT_MESH_FILE *  UNIT  * NO_MESH *  MESHLESS *
       0                       0               0                 1
* POST_DATA_FILE * ELEM_OUT * NODE_OUT *NUMBER_OUTPUT_MATS * AVERAGE * WIDE * SUF_OPTION *
        0               0        0           0
* MESH * CURRENT * MAGNETIC * FORCE_J_B * FORCE_NODAL * DISP * ELEM * HEAT * MAGNETIZATION * IRON_LOSS *
   0        0         0            0          0             0            0
*   MESH   *   A   *   V   *   B   *   B_INTEG *    J_Q  *
     0         0       0       0         0           0
*  Q_AVERAGE * HEAT  *  MAG_FLUX  * CUR_FLUX *
        0         0            0            0
* FORCE_J_B * FORCE_NODAL * MAGNETIC_ENERGY * IRON_LOSS *
        0         0
* GEOMETRY * DELTA_Z(m) or DETLA_THETA(deg)* NO_LAYERS *
     0         1.0
*COORDINATE * NO_COORDINATES *
COORDINATE         0
* FAR_BOUNDARY_CONDITION 
        0                     0               
* DISTANCE_JUDGE(m) * Distance for judgement (m)
      1.e-3
* NO_BN0_PLANES *
    0
* NO_HT0_PLANES *
    0
* NO_A0_LINE *
    0
* CYCLIC  *  SYMMETRICITY * DIVISION * SURFACE_MAT_ID * FITTNESS * LINE_INPUT * N_CYCLIC *
     0               1             0          11
* NO_MAT_IDS *  EXTEND_TOTAL *  NO_SMAT_IDS 
     0               0            0
*SOURCE *
SOURCE  
*NETWORK * REGION_FACTOR *
NETWORK   1    
*VPS * ID * NODE1 * NODE2 * TIME_ID *
VPS     1     1    2       1
*R   * ID * NODE1 * NODE2 * RESISTANCE *
R         2     2    3      100.
*L   * ID * NODE1 * NODE2 * INDUCTANCE *
L        3      3     4     1.
*C   * ID * NODE1 * NODE2 * CAPACITANCE *
C       4       4     1     0.00001
*END *
END
*END of SOURCE *
END
* NO_DATA *
      1
* TIME_ID * OPTION *
      1     0
*   C0    *   C1    *   C2    *   C3     *   C4     *  C5    *   C6    *
      100.      0.0       0.0          0       -100.0         0.0       0.0
*  TEXP   *   TCYCLE  *
   0.0         0.001